SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	1A
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

55

93

------

23cm	0.0

0.5

1.0

1.5

Yellowish brown gravelly silty sand

Yellowish brown sand with silt

Refusal strata in the form of Conglomerate

35

0

23

40

87

21

25

13

42

0

0

14

Non

Non

33

Plastic

Plastic

21
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3	B.H. No. : 1A
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Brownish red Conglomerate

-

9

0

0

19

0

60
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	2A
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

26

30

-----

6cm	0.0

0.5

0.8

1.0

Yellowish brown gravelly silty sand

Change of the strata

Refusal strata in the form of Conglomerate

52

41

7

0

Non

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3	B.H. No. : 2A
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

3.0	-

Yellowish pinkish grey Conglomerate

-

Yellowish pinkish grey Conglomerate

-

0

9

0

0

0

0

0

31

0

0

55

25
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	3A
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

41

51

31

------

5cm	0.0

0.5

1.0

1.5

2.0

Yellowish brown silty sand with gravel

Gravelly silty sand

Refusal strata in the form of Conglomerate

3

39

74

34

23

27

0

0

Non

Non

Plastic

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3	B.H. No. : 3A
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
2.0

3.0	-

Whitish/ pinkish brownish grey

Conglomerate

-

9

0

0

27

0

27
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	4A
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

57

-----

15cm

35

----

3cm	0.0

0.5

1.0

Yellowish brown gravelly sand with silt

Refusal strata in the form of Sandstone

60

29

11

0

Non

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 4A
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

1.5

3.0	-

Pinkish whitish grey Sandstone

-

Brownish red Sandstone

-

4

14

0

0

0

0

26

23

0

0

25

70

Highly

weathered
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	5
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

39

33

------

5cm

0.0

0.5

1.0

1.5

Yellowish brown sand with silt

Refusal strata in the form of Sandstone

0

57

10

0

Non

Plastic

1.82

3.5

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 5
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0

-

Whitish pinkish grey Sandstone

-

23

0

0

45

0

70

Highly

weathered
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	6
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

66

------

15cm	0.0

0.5

1.0

Yellowish brown silty sand with gravel

Refusal strata in the form of Conglomerate

1.70

6.4
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 6
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

3.0	-

Whitish pinkish grey Conglomerate

-

Whitish pinkish grey Conglomerate

-

0

4

0

0

0

0

0

20

0

0

24

14

N=29/5cm

at 2.5m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	7
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

50

31

-----

5cm	0.0

0.5

1.0

1.5

Yellowish brown gravelly silty sand

Refusal strata in the form of Sandstone

35

39

26

0

Non

Tube

Plastic

bent
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 7
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Whitish pinkish red Sandstone

-

17

0

0

18

0

40

Highly weathered
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	8
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

69

------

15cm

0.0

0.5

0.8

1.0

Yell. brown gravelly sand with traces of silt

Change of the strata

Refusal strata in the form of Conglomarate

36

60

4

0

Low

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 8
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

3.0	-

Yellowish pinkish grey Conglomerate

-

Yellowish pinkish grey Conglomerate

-

0

3

0

0

0

0

0

32

0

0

28

20

N=31/5cm

at 2.5m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	9
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

58

51

-----

15cm	0.0

0.5

0.8

1.0

1.3

1.5

Yellowish brown gravelly sand with silt

Change of the strata

Yellowish brown sand with traces of silt

Change of the strata

Refusal strata in the form of Conglomerate

34

0

48

95

18

5

0

0

Non

Non

Plastic

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 9
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Yellowish pinkish grey Conglomerate

-

0

0

0

0

0

25

N=31/5cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	10
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

32

114	0.0

0.5

1.0

1.3

1.5

2.0

Yellowish brown gravelly silty sand

Change of the strata

Yell. brown gravelly sand with traces of silt

Refusal strata in the form of Conglomarate

42

55

42

36

16

9

0

0

Non

Non

Plastic

Plastic

4.5

1.69
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 10
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
2.0

3.0	-

Whitish yellowish greyish brown Conglomerate

-

0

0

0

0

0

18

N=31/5cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	11
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

47

32

------

8cm	0.0

0.5

1.0

1.5

Yellowish br. gravelly sand with traces of silt

Yellowish brown gravelly sand with silt

Refusal strata in the form of Conglomerate

55

20

38

69

7

11

0

0

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 11
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Whitish yellowish brownish grey Conglomerate

-

7

0

0

11

0

30
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	12
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

56

-----

12cm	0.0

0.5

1.0

Yellowish brown gravelly silty sand

Refusal strata in the form of Conglomerate

1.63

4.9
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 12
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

3.0

-

Whitish yellowish brownish grey conglomerate

-

Whitish yellowish brownish grey Conglomerate

-

0

0

0

0

0

0

0

0

0

0

25

10	N=27/5cm

at 2.5m depth

N=31/5cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3	B.H. No.:	13
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

37

58

-----

13cm	0.0

0.5

1.0

1.5

Yellowish brown silty sand with gravel

Refusal strata in the form of Sandstone

9

61

30

0

Low

Plastic

1.84

13.7
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 13
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Greyish white Sandstone

-

12

0

0

44

0

80

Highly

weathered
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	14
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

34

-------

5cm	0.0

0.5

1.0

Yellowish brown gravelly silty sand

Refusal strata in the form of Sandstone

35

50

15

0

Non

Plastic

1.71

9.2
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 14
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

3.0	-

Pinkish whitish grey Sandstone

-

Pinkish whitish grey Sandstone

-

18

8

0

0

0

0

40

66

0

0

60

25

Moderately

weathered
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	15
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

52

51

-----

13cm	0.0

0.5

1.0

1.5

Yellowish brown silty sand with gravel

Refusal strata in the form of Conglomerate

8

69

23

0

Non

Plastic

1.75

6.4
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 15
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Whitish pinkish brown Conglomerate

-

0

0

0

0

0

32	N=32/5cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	16
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

52

61

-----

15cm	0.0

0.5

1.0

1.3

1.5

2.0

Yellowish brown gravelly sand with silt Yellowish brown gravelly silty sand

Change of the strata

Yell. brown sand with traces of silt and gravel

Refusal strata in the form of Sandstone

40

46

7

45

33

89

15

21

4

0

0

0

Non

Non

Non

Plastic

Plastic

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 16
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
2.0

3.0	-

Reddish brown Sandstone

-

0

0

0

0

0

20

N=30/8cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	17
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

47

29

------

5cm	0.0

0.5

0.8

1.0

1.5

Yellowish brown gravelly silty sand

Change of the strata

Yell. brown sand with traces of silt and gravel

Refusal strata in the form of Conglomerate

30

10

49

81

21

9

0

0

Non

Non

Plastic

Plastic
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 17
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Whitish pinkish grey Conglomerate

-

0

0

0

0

0

20	N=29/6cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	18
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

102	0.0

0.5

0.8

1.0

Yell. brown gravelly sand with traces of silt

Change of the strata

Refusal strata in the form of Conglomarate

67

29

4

0

Non

Plastic

ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 18
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

3.0	-

Whitish pinkish grey Conglomerate

-

Whitish pinkish grey Conglomerate

-

0

0

0

0

0

0

0

0

0

0

21

9

N=31/8cm

at 2.5m depth

N=29/5cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	19
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

30

59

-----

13cm	0.0

0.5

0.8

1.0

1.5

Yellowish brown gravelly sand with silt

Change of the strata

Yell.brown sand with traces of silt and gravel

Refusal strata in the form of Sandstone

25

9

60

88

15

3

0

0

Non

Non

Plastic

Plastic
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 19
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Greyish white Sandstone

-

0

0

0

0

0

25

N=31/3cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	20
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

37

114	0.0

0.5

1.0

1.3

1.5

1.8

2.0

Yellowish gravelly sand with silt

Change of the strata

Yellowish brown sand with traces of silt

Change of the strata

Refusal strata in the form of Conglomarate

33

0

47

91

20

9

0

0

Non

Non

Plastic

Plastic

1.60

2.4
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 20
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
2.0

3.0	-

Pinkish whitish grey Conglomerate

-

0

0

0

0

0

35	N=29/5cm

at 3m depth
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	4m	B.H. No.:	21
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

26

40

58

55

34

—

5cm	0.0

0.5

1.0

1.5

2.0

2.5

3.0

3.5

4.0

Yellowish brown sand with traces of silt

Yellowish brown sand with traces of silt

Yellowish brown sand with traces of silt

Yellowish brown sand with traces of silt

Conglomerate

0

0

0

0

91

95

98

98

9

2

2

2

0

0

0

0

Non

Non

Non

Non

Plastic

Plastic

Plastic

Plastic

1.82

1.90

1.92

17.8

19.9

18.6
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	28
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

64

64

—

15cm	0.0

0.5

1.0

1.3

1.5

Yellowish brown silty sand with gravel

Change of the strata

Conglomerate

12

0

57

91

31

9

0

0

Non

Non

Plastic

Plastic
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 28
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Pinkish brown white conglomerate

-

14

0

0

16

0

27
SOIL PROFILE	Project :	Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan
B.H. Location :	Water Table :	N.E.	Term. Depth :	3m	B.H. No.:	29
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

47

32

-----

5cm	0.0

0.5

1.0

1.5

Yellowish brown sand with traces of silt

Yellowish brown sand with traces of silt

Refusal Strata (Reddish/ whitish grey Sandstone

0

0

93

98

7

2

0

0

Non

Non

Plastic

Plastic
ROCK PROFILE	Project : Proposed Project 375MW ACME Village Rampuriya, Tehsil Sahgada, Dist Jaisalmer, Rajasthan	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3m	B.H. No. : 29
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.5

3.0	-

Reddish/ whitish grey Sandstone

-

16

1

0

44

7

45