NCD/Q/GLBPL/193/2022	22 March 2023

Good Luck Buildtech Pvt Ltd.,

Email : nayab.hasan@hiparks.com

Kind Attn : Mr. Hasan

Sub :	Conducting Modulus of Sub-grade Reaction Test

Dear Sir,

This is in reference to the above mentioned subject , please find hereunder our offer along with terms and conditions for the same.

SCHEDULE OF ITEM AND RATES

1.	Mobilisation of equipment and personnel to the site for carrying out the following field investigations.

2.	Conducting modulus of sub grade reaction (K-value test) on the made up surface as per IS : 9214 (1979) .

The plate load test shall be conducted to determine the K-value only and shall be conducted on a 30 x 30cm plate, subjecting the plate to a maximum loading intensity of 4 kg/cm2 or 25mm settlement whichever occurs earlier.

10 Nos. @ Rs. 25,000/= per test @ Rs. 2,50,000/=

3.	Professional consulting fees inclusive of preparation and submission of technical report .

Note :	The above rates have been quoted considering minimum 2 tests shall be conducted in one mobilisation.

TERMS AND CONDITIONS

1.	As per the notification of central government GST @ 18% shall be charged extra on the billed amount.

2.	We require a prior notice of 1 week to mobilise the team and submission of the report.

3.	As the tests are to be conducted on the plain level surface heavy vehicle for reaction loading shall be arranged by the clients.

4.	Minimum 2 tests shall be cleared at a time.

5.	The site should be free from any encumbrances and should be in full possession of the clients. Test locations at site shall be shown to us by one of your representatives.

Thanking you

yours sincerely

Y.S. Rana

Executive Consultant