SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	6.5m	B.H. No.:	1
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

15

19

27

------

3cm	0.0

0.9

1.5

2.4

3.0

3.5

Brownish grey clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Refusal/ rock strata (Yel. grey Sandstone)

4

7

35

34

50

45

11

14

27

31

19

21

2.02

2.05

23.5

12.1

CD

0.12

27
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 6.5m	B.H. No. : 1
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
3.5

5.0

6.5	-

Whitish/ yellowish/pinkish grey Sandstone

-

Whitish/ yellowish/pinkish grey Sandstone

-

12

10

0

0

0

0

31

27

0

0

80

95

2.30

3.8

3.9

1040

Highly weathered rock
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.5m	B.H. No.:	2
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

12

23

35

-------

5cm	0.0

0.9

1.5

2.4

3.0

3.5

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Refusal/ rock strata (Brownish yellow Sandstone)

7

13

30

30

49

46

14

11

30

29

20

20

1.96

1.98

15.1

17.6

CD

0.13

26
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.9m	B.H. No.:	3
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

13

46

------

15cm

28

------

5cm	0.0

0.9

1.5

2.4

3.0

3.9

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Refusal/ rock strata (Brownish yellow Sandstone)

18

10

23

35

46

45

13

10

26

24

18

16

1.80

8.1
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	10m	B.H. No.:	4
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

16

23

32

55

66

-----

20cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

7.0

Greyish brown clayey sandy silt with gravel

Greyish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown silty sand with gravel

Yellowish brown clayey silty sand with gravel

Refusal/ rock strata (Brownish grey Sandstone)

13

19

10

3

26

27

54

44

49

42

36

43

12

12

0

10

32

25

Low

24

21

17

Plastic

17

1.89

1.90

1.74

Tube

9.9

13.2

2.8

bent

CD

CD

0.12

0.09

27

29
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 10	B.H. No. : 4
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
7.0

8.5

10.0	-

Whitish/ yellow/ pinkish grey Sandstone

-

Whitish/ yellow/ pinkish grey Sandstone

-

9

10

0

1

0

0

14

34

0

7

80

90

2.45

2.4

1.8

1170

N=31/4cm

at 8.5m depth

Highly weathered rock
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.5m	B.H. No.:	5
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

17

38

32

-----

5cm	0.0

0.9

1.5

2.4

3.0

3.5

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Refusal/ rock strata (Brownish yellow Sandstone)

22

6

29

33

37

46

12

15

25

29

17

20

2.08

1.98

12.1

14.9

CD

0.13

28

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	10m	B.H. No.:	6
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

26

41

39

48

78

31

------

8cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

6.9

7.5

8.5

Yellowish brown clayey sandy silt with gravel

Change of the strata

Yellowish brown silty sand with gravel

Change of the strata

Yellowish brown clayey sandy silt

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt

Refusal/ rock strata (Br. grey Sandstone)

5

10

0

4

0

32

57

44

43

23

48

33

45

44

62

15

0

11

9

15

30

Non

25

24

32

20

Plastic

17

16

21

2.00

2.04

2.00

1.95

Tube

8.7

8.9

14.0

9.6

bent

CD

CD

0.07

0.11

29

30
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 10m	B.H. No. : 6
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
8.5

10.0	-

Whitish/ yellowish/ pinkish grey Sandstone

-

10

0

0

17

0

80

2.42

3.7

2.7

325

Highly weathered rock

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	5m	B.H. No.:	7
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

53

29

41

29

-----

3cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.0

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Refusal/ rock strata (Brownish yellow Sandstone)

18

3

2

25

33

44

45

52

45

12

12

9

30

29

23

20

20

16

2.10

2.04

2.07

16.1

16.5

15.5

CD

0.12

28
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	4.2m	B.H. No.:	8
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

32

------

4cm	0.0

0.9

1.2

Brownish grey clayey silty sand

Refusal/ rock strata (Brownish grey Sandstone)

1.90

6.6

ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4.2m	B.H. No. : 8
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.2

2.7

4.2	-

Yellowish/ whitish/ pinkish grey Sandstone

-

Yellowish/ whitish/ pinkish grey Sandstone

-

12

3

1

6

0

1

31

87

7

74

45

90

2.44

4.8

3.9

601

Highly weathered rock

Moderately to more or less sound rock
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.3m	B.H. No.:	9
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

31

-----

3cm	0.0

0.3	Yellowish brown clayey sandy silt

Refusal/ rock strata (Brownish grey Sandstone)
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3.3m	B.H. No. : 9
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.3

1.8

3.3	-

Yellowish/ whitish/ pinkish grey Sandstone

-

Yellowish/ whitish/ pinkish grey Sandstone

-

10

8

0

1

0

0

17

31

0

8

75

90

2.51

2.6

1.9

392

Highly weathered rock

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	6.5m	B.H. No.:	10
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

31

22

34

-----

3cm	0.0

0.9

1.5

2.4

3.0

3.5

Greyish brown clayey sandy silt with gravel

Greyish brown clayey sandy silt with gravel

Refusal/ rock strata (Yellowish/ pinkish grey Sandstone)

10

2

25

36

49

47

16

15

31

29

20

20

2.03

2.02

10.4

11.6

CD

0.13

27
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 6.5m	B.H. No. : 10
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
3.5

5.0

6.5	-

Yellowish/ pinkish grey Sandstone

-

Yellowish/ pinkish grey Sandstone

-

10

6

3

4

0

2

73

96

41

74

85

90

2.39

3.9

2.9

470

Moderately weathered to more or less sound rock

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	2.5m	B.H. No.:	11
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

28

27

-----

3cm	0.0

0.9

1.5

2.5

Brownish grey clayey sandy silt with gravel

Refusal/ rock strata (Brownish grey Sandstone)

7

37

43

13

27

19

1.84

6.9

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	4m	B.H. No.:	12
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

35

-----

5cm	0.0

1.0	Yellowish brown clayey sandy silt with gravel

Refusal/ rock strata (Brownish grey Sandstone)

ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 12
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
1.0

2.5

4.0	-

Whitish/ yellow/ pinkish grey Sandstone

-

Whitish/ yellow/ pinkish grey Sandstone

-

10

12

1

1

0

0

42

45

12

7

70

110

2.52

4.8

3.5

643

Highly weathered to moderately weathered rock

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	5m	B.H. No.:	13
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

17

24

31

34

-----

5cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.0

Brownish yellow silty sand with gravel

Change of the strata

Brownish yellow clayey sandy silt with gravel

Change of the strata

Brownish yellow clayey silty sand with gravel

Refusal/ rock strata (Brownish grey Sandstone)

12

6

2

51

27

51

37

53

38

0

14

9

Low

30

23

Plastic

20

16

1.78

1.95

2.09

6.2

9.2

17.6

CD

0.13

28
SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	9.5m	B.H. No.:	14
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

15

21

24

25

28

25

30

-----

3cm	0.0

0.9

1.5

2.4

3.0

3.9

4.3

4.5

5.4

6.0

6.9

7.5

8.4

9.0

9.5

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Change of the strata

Brownish yellow silty sand with gravel

Brownish yellow silty sand with gravel

Change of the strata

Brownish yellow clayey sandy silt

Brownish grey clayey sandy silt with gravel

Refusal/ rock strata (Brownish grey Sandstone)

13

7

15

29

0

2

37

44

47

45

19

23

40

39

38

26

67

63

10

10

0

0

14

12

26

25

Low

Non

30

27

18

17

Plastic

Plastic

21

19

1.90

1.99

2.07

1.93

2.17

1.97

7.7

8.6

10.3

6.1

13.8

13.4

CD

CD

0.11

0.07

27

28
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4.5m	B.H. No. : 15
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.5

3.0

4.5	-

Whitish/ reddish brownish grey Sandstone

-

Whitish/ reddish brownish grey Sandstone

-

Whitish/ reddish brownish grey Sandstone

-

24

22

8

1

4

6

0

0

0

56

89

83

8

28

60

90

105

100

2.51

3.9

2.8

479

Moderately weathered rock

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.3m	B.H. No.:	16
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

34

-----

3cm	0.0

0.3

Yellowish brown clayey sandy silt with gravel

Refusal/ rock strata ( Brownish grey Sandstone)

ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 3.3m	B.H. No. : 16
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.3

1.5

3.3	-

Whitish/ yellowish/ pinkish grey Sandstone

-

Whitish/ yellowish/ pinkish grey Sandstone

-

12

14

0

0

0

0

28

32

0

0

75

85

3.42

3.9

2.8

575

Highly weathered rock

ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4.5m	B.H. No. : 17
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.5

3.0

4.5	-

Pinkish/ whitish/ brownish grey Sandstone

-

Pinkish/ whitish/ brownish grey Sandstone

-

Pinkish/ whitish/ brownish grey Sandstone

-

16

10

7

3

2

1

0

1

0

0

0

1

80

86

88

27

46

73

90

105

110

2.47

3.8

2.7

639

Moderately weathered to more or less sound rock
ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4.5m	B.H. No. : 18
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.5

3.0

4.5	-

Pinkish/ whitish/ brownish grey Sandstone

-

Pinkish/ whitish/ brownish grey Sandstone

-

Pinkish/ whitish/ brownish grey Sandstone

-

13

18

8

4

2

5

0

1

1

66

89

96

38

34

69

85

100

105

2.62

5.1

3.9

727

Moderately weathered to more or less sound rock

ROCK PROFILE	Project : Proposed Project at Malanpur MPIDC Industrial Area, Gwalior	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4.5m	B.H. No. : 19
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.5

3.0

4.5	-

Pinkish/ whitish/ brownish grey Sandstone

-

Pinkish/ whitish/ brownish grey Sandstone

-

Pinkish/ whitish/ brownish grey Sandstone

-

17

21

11

2

3

6

0

0

0

64

98

99

21

30

60

85

105

110

3.44

4.8

3.3

765

Moderately weathered rock

SOIL PROFILE	Project :	Proposed Project at Malanpur MPIDC Industrial Area, Gwalior
B.H. Location :	Water Table :	N.E.	Term. Depth :	5m	B.H. No.:	20
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

13

17

22

34

-----

5cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.0

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Brownish yellow clayey sandy silt with gravel

Refusal/ rock strata (Br. grey Sandstone)

9

5

29

25

22

29

45

53

31

21

20

11

34

35

26

22

22

18

2.00

1.90

2.03

10.6

7.3

10.6

CD

0.14

27