SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	Term. Depth :	B.H. No.:
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 1
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish/ brownish grey clayey sandy silt

6

8

9

0

0

0

0

0

0

13

13

14

0

0

0

28

48

52	N=50/10cm

at 1m depth

N=79/20cm

at 2.5m depth

N=35/5cm

at 4m depth
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 2
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish/ brownish grey clayey sandy silt

5

9

7

0

0

0

0

0

0

9

12

11

0

0

0

33

49

58	N=71/20cm

at 1m depth

N=41/5cm

at 2.5m depth

N=32/3cm

at 4m depth
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	4.5m	B.H. No.:	3
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

8

10

62

36

-----

5cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

Yellowish grey sandy silty clay with gravel

Yellowish grey sandy clayey silt

Yellowish grey clayey sandy silt with gravel

Refusal/rock strata (Yellowish grey highly weathered Deccan Trap)

Observed 'N' Values

2

0

3

11

6

44

36

59

45

51

35

8

80

77

40

45

43

26

1.95

2.03

26.0

33.6

CD

0.28

22
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.9m	B.H. No.:	4
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

12

55

63

------

15cm	0.0

0.9

1.5

2.4

3.0

3.9

Yellowish grey sandy clayey silt

Yellowish grey clayey sandy silt with gravel

Refusal/ rock strata (Yellowish grey highly weathered Deccan Trap)

Observed 'N' Values

0

3

9

42

61

47

30

8

71

55

42

33

1.93

1.96

32.8

32.7

CD

0.26

22
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 5
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish/ brownish grey clayey sandy silt

5

7

7

0

0

0

0

0

0

9

13

10

0

0

0

26

46

57	N=36/3cm

at 1m depth

N=60/10cm

at 2.5m depth

N=40/7cm

at 4m depth
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	10m	B.H. No.:	6
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

12

36

38

51

47

64

-----

15cm

0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

6.9

7.5

8.5

Yellowish brown sandy clayey silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Refusal/ rock strata (Yellowish/ brownish grey highly weathered Deccan Trap)

Observed 'N' Values

8

2

5

9

20

10

8

13

26

30

54

83

72

59

48

28

7

10

6

2

88

89

70

60

54

47

50

45

40

36

2.03

2.06

2.14

2.19

2.02

33.8

32.7

28.6

36.9

20.9

CD

CD

0.30

0.25

23

28
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 10	B.H. No. : 6
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
8.5

10.0	-

Yellowish/ brownish grey highly weathered Deccan Trap

-

0

0

0

0

0

42	N=42/7cm

at 10m depth

SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	6m	B.H. No.:	7
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

10

17

20

70

61

----

13cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.4

6.0

Yellowish grey sandy clayey silt with gravel

Reddish brown sandy clayey silt with gravel

Yellowish brown sandy clayey silt

Yellowish grey sandy clayey silt

Refusal/ rock strata ( Yellowish grey highly weathered Deccan Trap)

Observed 'N' Values

9

2

0

2

17

3

69

61

93

20

20

4

68

65

73

40

39

41

2.05

2.08

2.10

23.2

24.2

32.4

CD

0.27

24
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.5m	B.H. No.:	8
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

12

72

38

-----

5cm	0.0

0.9

1.5

2.3

2.4

3.0

3.5

Yellowish grey sandy clayey silt with gravel

Change of the strata

Yellowish grey clayey silty sand with gravel

Refusal/ rock strata (Yellowish grey highly weathered Deccan Trap)

Observed 'N' Values

4

2

13

33

43

59

40

6

82

71

44

38

1.95

1.78

15.1

15.2

CD

0.24

28
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 9
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish/ brownish grey clayey sandy silt

6

6

6

0

0

0

0

0

0

10

10

8

0

0

0

30

56

62	N=70/2cm

at 1m depth

N=65/18cm

at 2.5m depth

N=58/10cm

at 4m depth
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 10
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish/ brownish grey clayey sandy silt

6

8

7

0

1

0

0

0

0

14

19

13

0

0

0

27

65

62	N=64/12cm

at 1m depth

N=70/13cm

at 2.5m depth

N=42/5cm

at 4m depth
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	5m	B.H. No.:	11
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

7

19

16

32

----

3cm	0.0

0.9

1.5

2.4

3.0

3.9

4.5

5.0

Yellowish grey sandy silty clayey

Yellowish grey sandy clayey silt with gravel

Yellowish grey sandy clayey silt with gravel

Refusal/ rock strata (Yellowish grey highly weathered Deccan Trap)

Observed 'N' Values

0

3

2

11

8

3

44

80

50

45

9

45

77

71

80

47

40

48

2.00

2.07

2.15

33.2

31.2

35.4

CD

0.25

22
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	3.9m	B.H. No.:	12
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

46

40

30

----

3cm	0.0

0.9

1.5

2.4

3.0

3.9

Yellowish brown silty sand with gravel

Yellowish brown clayey silty sand with gravel

Refusal/ rock strata (Yellowish brown highly weathered Deccan Trap)

Observed 'N' Values

29

10

44

55

27

29

0

6

Low

Low

Plastic

Plastic

1.97

2.04

23.0

28.3

CD

0.14

29
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	8m	B.H. No.:	13
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

25

19

17

24

34

56

-----

10cm	0.0

0.9

1.5

2.0

2.4

3.0

3.9

4.5

5.4

6.0

6.9

8.0

Yellowish brown silty sand with gravel

Change of the strata

Yell./ whitish grey sandy clayey silt with gravel

Yell./ whitish grey sandy clayey silt

Yellowish brown clayey sandy silt with gravel

Yellowish brown clayey sandy silt with gravel

Refusal/ rock strata ( Yellowish/ whitish grey highly weathered Deccan Trap)

Observed 'N' Values

20

3

0

2

2

57

22

5

13

11

23

38

60

78

85

0

37

35

7

2

Low

84

94

72

74

Plastic

47

53

40

42

1.98

2.05

2.15

2.05

24.5

31.1

31.7

27.2

CD

0.27

23
ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 5.5m	B.H. No. : 14
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
`0.0

1.0

2.5

4.0

5.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Boulder Strata

-

Bouldery Strata : Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish brown clayey sandy silt

7

10

8

10

0

0

0

0

0

0

0

0

15

15

12

19

0

0

0

0

32

45

49

57	N=55

at 1m depth

N=63/2cm

at 2.5m depth

N=46/5cm

at 4m depth

N=55/5cm

at 5.5m depth

ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 5.5m	B.H. No. : 15
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0

5.5	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish brown clayey sandy silt

5

8

8

11

0

0

0

0

0

0

0

0

11

12

17

16

0

0

0

0

28

44

47

54	N=40/6cm

at 1m depth

N=64/10cm

at 2.5m depth

N=84/20cm

at 4m depth

N=44/5cm

at 5.5m depth

ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 5.5m	B.H. No. : 16
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0

5.5	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish brown clayey sandy silt

6

11

8

9

0

0

0

0

0

0

0

0

12

16

12

15

0

0

0

0

30

49

6

60	N=30/1cm

at 1m depth

N=57/10cm

at 2.5m depth

N=38/5cm

at 4m depth

N=42/5cm

at 5.5m depth

ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 5.5m	B.H. No. : 17
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0

5.5	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish brown clayey sandy silt

6

7

10

9

0

0

0

0

0

0

0

0

11

12

18

14

0

0

0

0

35

48

53

60	N=34/3cm

at 1m depth

N=38/4cm

at 2.5m depth

N=56/5cm

at 4m depth

N=46/5cm

at 5.5m depth

SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	8m	B.H. No.:	18
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

73

------

25cm

46

40

53

45

42

-------

7cm	0.0

0.9

1.0

2.0

2.5

3.9

4.5

5.4

6.0

6.9

7.5

8.0

Yellowish brown clayey sandy silt intermixed with gravel, pebbles, cobbles and occasional boulders

Change of the strata

Yellowish brown clayey sandy silt with gravel

Yell./ whitish grey sandy clayey silt with gravel

Yellowish brown clayey sandy silt with gravel

Yellowish brown sandy clayey silt with gravel

Refusal/ rock strata (Yellowish/ whitish brown highly weathered Deccan Trap)

Observed "N' Values

5

3

7

6

39

9

19

17

48

54

69

37

8

34

5

40

48

88

54

86

27

48

36

47

2.12

2.18

2.00

30.1

34.4

21.9

CD

0.28

27
SOIL PROFILE	Project :	Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh
B.H. Location :	Water Table :	N.E.	Term. Depth :	10m	B.H. No.:	19
Soil Description
Grain Size Analysis	Atterberg

Limits	In-situ properties	Triaxial Test

9

38

39

74

------

25cm

36

-----

3cm

4.0

5.5

7.0

8.5

10.0	From 0m to 4m depth Continued in Rock Profile Tables

Yellowish brown sandy silty clay with gravel

Yellowish brown sandy clayey silt with gravel

Yellowish brown sandy clayey silt with gravel

Yell. whitish grey highly weathered rock

Refusal/ rock strata (Yellowish / whitish grey highly weathered Deccan Trap)

Observed 'N' Values

13

12

2

12

11

8

28

63

78

47

14

12

91

80

75

51

44

40

ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 10m	B.H. No. : 19
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish brown clayey sandy silt

5

6

6

0

0

0

0

0

0

14

10

10

0

0

0

22

57

62	N=58/10cm

at 1m depth

N= 98/5cm

at 2.5m depth

ROCK PROFILE	Project : Proposed Project At Vikram Udyogpuri, Indore, Madhya Pradesh	Location :
B.H. Size : Nx	Water Table (m): N.E.	Term. Depth (m): 4m	B.H. No. : 20
Strata Description	No. of Core Pieces of Size (cm)	Core Recovery (%)
Remarks
0.0

1.0

2.5

4.0	-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata

-

Bouldery Strata :: Gravel, pebbles, cobbles and occasional boulders intermixed with Yellowish brown clayey sandy silt

6

8

7

0

1

0

0

0

0

14

19

13

0

0

0

27

65

62	N=64/12cm

at 1m depth

N=70/13cm

at 2.5m depth

N=42/5cm

at 4m depth